(kicad_symbol_lib (version 20211014) (generator desktop_companion)
  (symbol "U1" (pin_names (offset 0.6)) (in_bom yes) (on_board yes)
    (property "Reference" "U" (at 0 19.78 0))
    (property "Value" "Seeed_XIAO_ESP32S3_nonSense" (at 0 21.78 0))
    (symbol "U1_0_1")
    (symbol "U1_1_1"
      (pin bidirectional line (at -2.54 16.51 0) (length 2.54)
        (name "D0_GPIO1")
        (number "1")
      )
      (pin bidirectional line (at -2.54 13.97 0) (length 2.54)
        (name "D1_GPIO2")
        (number "2")
      )
      (pin bidirectional line (at -2.54 11.430000000000001 0) (length 2.54)
        (name "D2_GPIO3_STRAP")
        (number "3")
      )
      (pin bidirectional line (at -2.54 8.89 0) (length 2.54)
        (name "D3_GPIO4")
        (number "4")
      )
      (pin bidirectional line (at -2.54 6.350000000000001 0) (length 2.54)
        (name "D4_GPIO5")
        (number "5")
      )
      (pin bidirectional line (at -2.54 3.8100000000000005 0) (length 2.54)
        (name "D5_GPIO6")
        (number "6")
      )
      (pin bidirectional line (at -2.54 1.2699999999999996 0) (length 2.54)
        (name "D6_GPIO43")
        (number "7")
      )
      (pin bidirectional line (at -2.54 -1.2699999999999996 0) (length 2.54)
        (name "D7_GPIO44")
        (number "8")
      )
      (pin bidirectional line (at -2.54 -3.8099999999999987 0) (length 2.54)
        (name "D8_GPIO7")
        (number "9")
      )
      (pin bidirectional line (at -2.54 -6.349999999999998 0) (length 2.54)
        (name "D9_GPIO8")
        (number "10")
      )
      (pin bidirectional line (at -2.54 -8.89 0) (length 2.54)
        (name "D10_GPIO9")
        (number "11")
      )
      (pin power_out line (at -2.54 -11.43 0) (length 2.54)
        (name "3V3_OUT")
        (number "12")
      )
      (pin power_in line (at -2.54 -13.969999999999999 0) (length 2.54)
        (name "GND")
        (number "13")
      )
      (pin power_in line (at -2.54 -16.509999999999998 0) (length 2.54)
        (name "VBUS_IN")
        (number "14")
      )
    )
  )
  (symbol "J1" (pin_names (offset 0.6)) (in_bom yes) (on_board yes)
    (property "Reference" "J" (at 0 7.08 0))
    (property "Value" "BQ24074_OUT" (at 0 9.08 0))
    (symbol "J1_0_1")
    (symbol "J1_1_1"
      (pin passive line (at -2.54 3.81 0) (length 2.54)
        (name "SYS_RAW")
        (number "1")
      )
      (pin passive line (at -2.54 1.27 0) (length 2.54)
        (name "GND")
        (number "2")
      )
    )
  )
  (symbol "J2" (pin_names (offset 0.6)) (in_bom yes) (on_board yes)
    (property "Reference" "J" (at 0 12.16 0))
    (property "Value" "DISPLAY_5206" (at 0 14.16 0))
    (symbol "J2_0_1")
    (symbol "J2_1_1"
      (pin passive line (at -2.54 8.89 0) (length 2.54)
        (name "+3V3")
        (number "1")
      )
      (pin passive line (at -2.54 6.35 0) (length 2.54)
        (name "GND")
        (number "2")
      )
      (pin passive line (at -2.54 3.8100000000000005 0) (length 2.54)
        (name "SPI_SCK")
        (number "3")
      )
      (pin passive line (at -2.54 1.2699999999999996 0) (length 2.54)
        (name "SPI_MOSI")
        (number "4")
      )
      (pin passive line (at -2.54 -1.2699999999999996 0) (length 2.54)
        (name "LCD_CS")
        (number "5")
      )
      (pin passive line (at -2.54 -3.8100000000000005 0) (length 2.54)
        (name "LCD_DC")
        (number "6")
      )
      (pin passive line (at -2.54 -6.350000000000001 0) (length 2.54)
        (name "LCD_RST")
        (number "7")
      )
      (pin passive line (at -2.54 -8.89 0) (length 2.54)
        (name "LCD_BL")
        (number "8")
      )
    )
  )
  (symbol "J3" (pin_names (offset 0.6)) (in_bom yes) (on_board yes)
    (property "Reference" "J" (at 0 8.35 0))
    (property "Value" "I2S_AUDIO_OPTION" (at 0 10.35 0))
    (symbol "J3_0_1")
    (symbol "J3_1_1"
      (pin passive line (at -2.54 5.08 0) (length 2.54)
        (name "+5V")
        (number "1")
      )
      (pin passive line (at -2.54 2.5399999999999996 0) (length 2.54)
        (name "GND")
        (number "2")
      )
      (pin passive line (at -2.54 0 0) (length 2.54)
        (name "I2S_BCLK")
        (number "3")
      )
      (pin passive line (at -2.54 -2.540000000000001 0) (length 2.54)
        (name "I2S_LRCLK")
        (number "4")
      )
      (pin passive line (at -2.54 -5.08 0) (length 2.54)
        (name "I2S_DIN")
        (number "5")
      )
    )
  )
  (symbol "J4" (pin_names (offset 0.6)) (in_bom yes) (on_board yes)
    (property "Reference" "J" (at 0 7.08 0))
    (property "Value" "POWER_SWITCH" (at 0 9.08 0))
    (symbol "J4_0_1")
    (symbol "J4_1_1"
      (pin passive line (at -2.54 3.81 0) (length 2.54)
        (name "SYS_FUSED")
        (number "1")
      )
      (pin passive line (at -2.54 1.27 0) (length 2.54)
        (name "SYS_SW")
        (number "2")
      )
    )
  )
  (symbol "J5" (pin_names (offset 0.6)) (in_bom yes) (on_board yes)
    (property "Reference" "J" (at 0 7.08 0))
    (property "Value" "S7V8F5_WIRED" (at 0 9.08 0))
    (symbol "J5_0_1")
    (symbol "J5_1_1"
      (pin passive line (at -2.54 3.81 0) (length 2.54)
        (name "SYS_SW")
        (number "1")
      )
      (pin passive line (at -2.54 1.27 0) (length 2.54)
        (name "GND")
        (number "2")
      )
      (pin passive line (at -2.54 -1.2699999999999996 0) (length 2.54)
        (name "+5V")
        (number "3")
      )
    )
  )
  (symbol "J6" (pin_names (offset 0.6)) (in_bom yes) (on_board yes)
    (property "Reference" "J" (at 0 7.08 0))
    (property "Value" "MOMENTARY_BUTTON" (at 0 9.08 0))
    (symbol "J6_0_1")
    (symbol "J6_1_1"
      (pin passive line (at -2.54 3.81 0) (length 2.54)
        (name "BUTTON_N")
        (number "1")
      )
      (pin passive line (at -2.54 1.27 0) (length 2.54)
        (name "GND")
        (number "2")
      )
    )
  )
  (symbol "J7" (pin_names (offset 0.6)) (in_bom yes) (on_board yes)
    (property "Reference" "J" (at 0 7.08 0))
    (property "Value" "CHARGER_PROGRAM_NTC" (at 0 9.08 0))
    (symbol "J7_0_1")
    (symbol "J7_1_1"
      (pin passive line (at -2.54 3.81 0) (length 2.54)
        (name "ISET")
        (number "1")
      )
      (pin passive line (at -2.54 1.27 0) (length 2.54)
        (name "GND")
        (number "2")
      )
      (pin passive line (at -2.54 -1.2699999999999996 0) (length 2.54)
        (name "NTC_TS")
        (number "3")
      )
    )
  )
  (symbol "J8" (pin_names (offset 0.6)) (in_bom yes) (on_board yes)
    (property "Reference" "J" (at 0 7.08 0))
    (property "Value" "103AT2_PACK_SENSOR" (at 0 9.08 0))
    (symbol "J8_0_1")
    (symbol "J8_1_1"
      (pin passive line (at -2.54 3.81 0) (length 2.54)
        (name "NTC_TS")
        (number "1")
      )
      (pin passive line (at -2.54 1.27 0) (length 2.54)
        (name "GND")
        (number "2")
      )
    )
  )
  (symbol "F1" (pin_names (offset 0.6)) (in_bom yes) (on_board yes)
    (property "Reference" "F" (at 0 7.08 0))
    (property "Value" "MF-MSMF110_16X-2" (at 0 9.08 0))
    (symbol "F1_0_1")
    (symbol "F1_1_1"
      (pin passive line (at -2.54 3.81 0) (length 2.54)
        (name "SYS_RAW")
        (number "1")
      )
      (pin passive line (at -2.54 1.27 0) (length 2.54)
        (name "SYS_FUSED")
        (number "2")
      )
    )
  )
  (symbol "D1" (pin_names (offset 0.6)) (in_bom yes) (on_board yes)
    (property "Reference" "D" (at 0 7.08 0))
    (property "Value" "SS14_SCHOTTKY" (at 0 9.08 0))
    (symbol "D1_0_1")
    (symbol "D1_1_1"
      (pin passive line (at -2.54 3.81 0) (length 2.54)
        (name "K")
        (number "1")
      )
      (pin passive line (at -2.54 1.27 0) (length 2.54)
        (name "A")
        (number "2")
      )
    )
  )
  (symbol "R1" (pin_names (offset 0.6)) (in_bom yes) (on_board yes)
    (property "Reference" "R" (at 0 7.08 0))
    (property "Value" "10k_1%" (at 0 9.08 0))
    (symbol "R1_0_1")
    (symbol "R1_1_1"
      (pin passive line (at -2.54 3.81 0) (length 2.54)
        (name "BUTTON_N")
        (number "1")
      )
      (pin passive line (at -2.54 1.27 0) (length 2.54)
        (name "+3V3")
        (number "2")
      )
    )
  )
  (symbol "R2" (pin_names (offset 0.6)) (in_bom yes) (on_board yes)
    (property "Reference" "R" (at 0 7.08 0))
    (property "Value" "10k_1%" (at 0 9.08 0))
    (symbol "R2_0_1")
    (symbol "R2_1_1"
      (pin passive line (at -2.54 3.81 0) (length 2.54)
        (name "LCD_CS")
        (number "1")
      )
      (pin passive line (at -2.54 1.27 0) (length 2.54)
        (name "+3V3")
        (number "2")
      )
    )
  )
  (symbol "R3" (pin_names (offset 0.6)) (in_bom yes) (on_board yes)
    (property "Reference" "R" (at 0 7.08 0))
    (property "Value" "10k_1%" (at 0 9.08 0))
    (symbol "R3_0_1")
    (symbol "R3_1_1"
      (pin passive line (at -2.54 3.81 0) (length 2.54)
        (name "LCD_RST")
        (number "1")
      )
      (pin passive line (at -2.54 1.27 0) (length 2.54)
        (name "+3V3")
        (number "2")
      )
    )
  )
  (symbol "R4" (pin_names (offset 0.6)) (in_bom yes) (on_board yes)
    (property "Reference" "R" (at 0 7.08 0))
    (property "Value" "3.57k_1%" (at 0 9.08 0))
    (symbol "R4_0_1")
    (symbol "R4_1_1"
      (pin passive line (at -2.54 3.81 0) (length 2.54)
        (name "ISET")
        (number "1")
      )
      (pin passive line (at -2.54 1.27 0) (length 2.54)
        (name "GND")
        (number "2")
      )
    )
  )
  (symbol "C1" (pin_names (offset 0.6)) (in_bom yes) (on_board yes)
    (property "Reference" "C" (at 0 7.08 0))
    (property "Value" "47uF_10V_X5R" (at 0 9.08 0))
    (symbol "C1_0_1")
    (symbol "C1_1_1"
      (pin passive line (at -2.54 3.81 0) (length 2.54)
        (name "+5V")
        (number "1")
      )
      (pin passive line (at -2.54 1.27 0) (length 2.54)
        (name "GND")
        (number "2")
      )
    )
  )
  (symbol "C2" (pin_names (offset 0.6)) (in_bom yes) (on_board yes)
    (property "Reference" "C" (at 0 7.08 0))
    (property "Value" "100nF_16V_X7R" (at 0 9.08 0))
    (symbol "C2_0_1")
    (symbol "C2_1_1"
      (pin passive line (at -2.54 3.81 0) (length 2.54)
        (name "COMPUTE_5V")
        (number "1")
      )
      (pin passive line (at -2.54 1.27 0) (length 2.54)
        (name "GND")
        (number "2")
      )
    )
  )
  (symbol "C3" (pin_names (offset 0.6)) (in_bom yes) (on_board yes)
    (property "Reference" "C" (at 0 7.08 0))
    (property "Value" "10uF_10V_X5R" (at 0 9.08 0))
    (symbol "C3_0_1")
    (symbol "C3_1_1"
      (pin passive line (at -2.54 3.81 0) (length 2.54)
        (name "+3V3")
        (number "1")
      )
      (pin passive line (at -2.54 1.27 0) (length 2.54)
        (name "GND")
        (number "2")
      )
    )
  )
  (symbol "C4" (pin_names (offset 0.6)) (in_bom yes) (on_board yes)
    (property "Reference" "C" (at 0 7.08 0))
    (property "Value" "100nF_16V_X7R" (at 0 9.08 0))
    (symbol "C4_0_1")
    (symbol "C4_1_1"
      (pin passive line (at -2.54 3.81 0) (length 2.54)
        (name "BUTTON_N")
        (number "1")
      )
      (pin passive line (at -2.54 1.27 0) (length 2.54)
        (name "GND")
        (number "2")
      )
    )
  )
  (symbol "C5" (pin_names (offset 0.6)) (in_bom yes) (on_board yes)
    (property "Reference" "C" (at 0 7.08 0))
    (property "Value" "47uF_10V_X5R" (at 0 9.08 0))
    (symbol "C5_0_1")
    (symbol "C5_1_1"
      (pin passive line (at -2.54 3.81 0) (length 2.54)
        (name "SYS_SW")
        (number "1")
      )
      (pin passive line (at -2.54 1.27 0) (length 2.54)
        (name "GND")
        (number "2")
      )
    )
  )
  (symbol "PWR_FLAG" (pin_names (offset 0)) (in_bom no) (on_board no)
    (property "Reference" "#FLG" (at 0 2.54 0))
    (property "Value" "PWR_FLAG" (at 0 5.08 0))
    (symbol "PWR_FLAG_1_1"
      (pin power_out line (at 0 0 90) (length 0)
        (name "pwr")
        (number "1")
      )
    )
  )
)
