(kicad_pcb (version 20221018) (generator desktop_companion)
(general (thickness 1.6)) (paper "A4")
(layers (0 "F.Cu" signal) (31 "B.Cu" signal) (36 "B.SilkS" user "b.silkscreen") (37 "F.SilkS" user "f.silkscreen") (38 "B.Mask" user) (39 "F.Mask" user) (41 "Cmts.User" user) (44 "Edge.Cuts" user) (47 "F.CrtYd" user) (49 "F.Fab" user))
(setup (pad_to_mask_clearance 0.05)) (net 0 "")
(net 1 "+3V3")
(net 2 "+5V")
(net 3 "BUTTON_N")
(net 4 "COMPUTE_5V")
(net 5 "GND")
(net 6 "I2S_BCLK")
(net 7 "I2S_DIN")
(net 8 "I2S_LRCLK")
(net 9 "ISET")
(net 10 "LCD_BL")
(net 11 "LCD_CS")
(net 12 "LCD_DC")
(net 13 "LCD_RST")
(net 14 "NTC_TS")
(net 15 "SPI_MOSI")
(net 16 "SPI_SCK")
(net 17 "SYS_FUSED")
(net 18 "SYS_RAW")
(net 19 "SYS_SW")
(net 20 "unconnected-(U1-D2_GPIO3_STRAP-Pad3)")
(footprint "DC:U1" (layer "F.Cu") (at 27.94 15.24)
(attr through_hole)
(fp_text reference "U1" (at 0 -11.6) (layer "F.SilkS"))
(fp_text value "Seeed_XIAO_ESP32S3_nonSense" (at 0 11.7) (layer "F.Fab"))
(pad "1" thru_hole circle (at -7.62 -7.62) (size 1.8 1.8) (drill 1.0) (layers "*.Cu" "*.Mask") (net 11 "LCD_CS"))
(pad "2" thru_hole circle (at -7.62 -5.08) (size 1.8 1.8) (drill 1.0) (layers "*.Cu" "*.Mask") (net 12 "LCD_DC"))
(pad "3" thru_hole circle (at -7.62 -2.54) (size 1.8 1.8) (drill 1.0) (layers "*.Cu" "*.Mask") (net 20 "unconnected-(U1-D2_GPIO3_STRAP-Pad3)"))
(pad "4" thru_hole circle (at -7.62 0.0) (size 1.8 1.8) (drill 1.0) (layers "*.Cu" "*.Mask") (net 13 "LCD_RST"))
(pad "5" thru_hole circle (at -7.62 2.54) (size 1.8 1.8) (drill 1.0) (layers "*.Cu" "*.Mask") (net 10 "LCD_BL"))
(pad "6" thru_hole circle (at -7.62 5.079999999999999) (size 1.8 1.8) (drill 1.0) (layers "*.Cu" "*.Mask") (net 3 "BUTTON_N"))
(pad "7" thru_hole circle (at -7.62 7.62) (size 1.8 1.8) (drill 1.0) (layers "*.Cu" "*.Mask") (net 6 "I2S_BCLK"))
(pad "8" thru_hole circle (at 7.62 7.62) (size 1.8 1.8) (drill 1.0) (layers "*.Cu" "*.Mask") (net 8 "I2S_LRCLK"))
(pad "9" thru_hole circle (at 7.62 5.079999999999999) (size 1.8 1.8) (drill 1.0) (layers "*.Cu" "*.Mask") (net 16 "SPI_SCK"))
(pad "10" thru_hole circle (at 7.62 2.54) (size 1.8 1.8) (drill 1.0) (layers "*.Cu" "*.Mask") (net 7 "I2S_DIN"))
(pad "11" thru_hole circle (at 7.62 0.0) (size 1.8 1.8) (drill 1.0) (layers "*.Cu" "*.Mask") (net 15 "SPI_MOSI"))
(pad "12" thru_hole circle (at 7.62 -2.54) (size 1.8 1.8) (drill 1.0) (layers "*.Cu" "*.Mask") (net 1 "+3V3"))
(pad "13" thru_hole circle (at 7.62 -5.08) (size 1.8 1.8) (drill 1.0) (layers "*.Cu" "*.Mask") (net 5 "GND"))
(pad "14" thru_hole circle (at 7.62 -7.62) (size 1.8 1.8) (drill 1.0) (layers "*.Cu" "*.Mask") (net 4 "COMPUTE_5V"))
)
(footprint "DC:J1" (layer "F.Cu") (at 5.08 12.7)
(attr through_hole)
(fp_text reference "J1" (at 0 -2.37) (layer "F.SilkS"))
(fp_text value "BQ24074_OUT" (at 0 5.01) (layer "F.Fab"))
(pad "1" thru_hole circle (at 0 0.0) (size 1.8 1.8) (drill 1.0) (layers "*.Cu" "*.Mask") (net 18 "SYS_RAW"))
(pad "2" thru_hole circle (at 0 2.54) (size 1.8 1.8) (drill 1.0) (layers "*.Cu" "*.Mask") (net 5 "GND"))
)
(footprint "DC:J2" (layer "F.Cu") (at 46.99 8.89)
(attr through_hole)
(fp_text reference "J2" (at 0 -2.3699999999999997) (layer "F.SilkS"))
(fp_text value "DISPLAY_5206" (at 0 20.25) (layer "F.Fab"))
(pad "1" thru_hole circle (at 0 0.0) (size 1.8 1.8) (drill 1.0) (layers "*.Cu" "*.Mask") (net 1 "+3V3"))
(pad "2" thru_hole circle (at 0 2.54) (size 1.8 1.8) (drill 1.0) (layers "*.Cu" "*.Mask") (net 5 "GND"))
(pad "3" thru_hole circle (at 0 5.08) (size 1.8 1.8) (drill 1.0) (layers "*.Cu" "*.Mask") (net 16 "SPI_SCK"))
(pad "4" thru_hole circle (at 0 7.62) (size 1.8 1.8) (drill 1.0) (layers "*.Cu" "*.Mask") (net 15 "SPI_MOSI"))
(pad "5" thru_hole circle (at 0 10.16) (size 1.8 1.8) (drill 1.0) (layers "*.Cu" "*.Mask") (net 11 "LCD_CS"))
(pad "6" thru_hole circle (at 0 12.7) (size 1.8 1.8) (drill 1.0) (layers "*.Cu" "*.Mask") (net 12 "LCD_DC"))
(pad "7" thru_hole circle (at 0 15.24) (size 1.8 1.8) (drill 1.0) (layers "*.Cu" "*.Mask") (net 13 "LCD_RST"))
(pad "8" thru_hole circle (at 0 17.78) (size 1.8 1.8) (drill 1.0) (layers "*.Cu" "*.Mask") (net 10 "LCD_BL"))
)
(footprint "DC:J3" (layer "F.Cu") (at 44.45 31.75)
(attr through_hole)
(fp_text reference "J3" (at 0 -2.3699999999999997) (layer "F.SilkS"))
(fp_text value "I2S_AUDIO_OPTION" (at 0 12.629999999999999) (layer "F.Fab"))
(pad "1" thru_hole circle (at 0 0.0) (size 1.8 1.8) (drill 1.0) (layers "*.Cu" "*.Mask") (net 2 "+5V"))
(pad "2" thru_hole circle (at 0 2.54) (size 1.8 1.8) (drill 1.0) (layers "*.Cu" "*.Mask") (net 5 "GND"))
(pad "3" thru_hole circle (at 0 5.08) (size 1.8 1.8) (drill 1.0) (layers "*.Cu" "*.Mask") (net 6 "I2S_BCLK"))
(pad "4" thru_hole circle (at 0 7.62) (size 1.8 1.8) (drill 1.0) (layers "*.Cu" "*.Mask") (net 8 "I2S_LRCLK"))
(pad "5" thru_hole circle (at 0 10.16) (size 1.8 1.8) (drill 1.0) (layers "*.Cu" "*.Mask") (net 7 "I2S_DIN"))
)
(footprint "DC:J4" (layer "F.Cu") (at 5.08 20.32)
(attr through_hole)
(fp_text reference "J4" (at 0 -2.37) (layer "F.SilkS"))
(fp_text value "POWER_SWITCH" (at 0 5.01) (layer "F.Fab"))
(pad "1" thru_hole circle (at 0 0.0) (size 1.8 1.8) (drill 1.0) (layers "*.Cu" "*.Mask") (net 17 "SYS_FUSED"))
(pad "2" thru_hole circle (at 0 2.54) (size 1.8 1.8) (drill 1.0) (layers "*.Cu" "*.Mask") (net 19 "SYS_SW"))
)
(footprint "DC:J5" (layer "F.Cu") (at 11.43 29.21)
(attr through_hole)
(fp_text reference "J5" (at 0 -2.37) (layer "F.SilkS"))
(fp_text value "S7V8F5_WIRED" (at 0 7.55) (layer "F.Fab"))
(pad "1" thru_hole circle (at 0 0.0) (size 1.8 1.8) (drill 1.0) (layers "*.Cu" "*.Mask") (net 19 "SYS_SW"))
(pad "2" thru_hole circle (at 0 2.54) (size 1.8 1.8) (drill 1.0) (layers "*.Cu" "*.Mask") (net 5 "GND"))
(pad "3" thru_hole circle (at 0 5.08) (size 1.8 1.8) (drill 1.0) (layers "*.Cu" "*.Mask") (net 2 "+5V"))
)
(footprint "DC:J6" (layer "F.Cu") (at 10.16 5.08)
(attr through_hole)
(fp_text reference "J6" (at 0 -2.37) (layer "F.SilkS"))
(fp_text value "MOMENTARY_BUTTON" (at 0 2.4699999999999998) (layer "F.Fab"))
(pad "1" thru_hole circle (at 0.0 0) (size 1.8 1.8) (drill 1.0) (layers "*.Cu" "*.Mask") (net 3 "BUTTON_N"))
(pad "2" thru_hole circle (at 2.54 0) (size 1.8 1.8) (drill 1.0) (layers "*.Cu" "*.Mask") (net 5 "GND"))
)
(footprint "DC:J7" (layer "F.Cu") (at 5.08 31.75)
(attr through_hole)
(fp_text reference "J7" (at 0 -2.37) (layer "F.SilkS"))
(fp_text value "CHARGER_PROGRAM_NTC" (at 0 7.55) (layer "F.Fab"))
(pad "1" thru_hole circle (at 0 0.0) (size 1.8 1.8) (drill 1.0) (layers "*.Cu" "*.Mask") (net 9 "ISET"))
(pad "2" thru_hole circle (at 0 2.54) (size 1.8 1.8) (drill 1.0) (layers "*.Cu" "*.Mask") (net 5 "GND"))
(pad "3" thru_hole circle (at 0 5.08) (size 1.8 1.8) (drill 1.0) (layers "*.Cu" "*.Mask") (net 14 "NTC_TS"))
)
(footprint "DC:J8" (layer "F.Cu") (at 20.32 41.91)
(attr through_hole)
(fp_text reference "J8" (at 0 -2.37) (layer "F.SilkS"))
(fp_text value "103AT2_PACK_SENSOR" (at 0 2.4699999999999998) (layer "F.Fab"))
(pad "1" thru_hole circle (at 0.0 0) (size 1.8 1.8) (drill 1.0) (layers "*.Cu" "*.Mask") (net 14 "NTC_TS"))
(pad "2" thru_hole circle (at 2.54 0) (size 1.8 1.8) (drill 1.0) (layers "*.Cu" "*.Mask") (net 5 "GND"))
)
(footprint "DC:F1" (layer "F.Cu") (at 10.16 12.7)
(attr smd)
(fp_text reference "F1" (at 0 2.805) (layer "F.SilkS"))
(fp_text value "MF-MSMF110_16X-2" (at 0 2.9050000000000002) (layer "F.Fab"))
(pad "1" smd rect (at -2.39 0) (size 1.68 2.95)  (layers "F.Cu" "F.Mask") (net 18 "SYS_RAW"))
(pad "2" smd rect (at 2.39 0) (size 1.68 2.95)  (layers "F.Cu" "F.Mask") (net 17 "SYS_FUSED"))
)
(footprint "DC:D1" (layer "F.Cu") (at 40.64 6.35)
(attr smd)
(fp_text reference "D1" (at 0 -2.495) (layer "F.SilkS"))
(fp_text value "SS14_SCHOTTKY" (at 0 2.5949999999999998) (layer "F.Fab"))
(pad "1" smd rect (at -1.905 0) (size 2.0 1.8)  (layers "F.Cu" "F.Mask") (net 4 "COMPUTE_5V"))
(pad "2" smd rect (at 1.905 0) (size 2.0 1.8)  (layers "F.Cu" "F.Mask") (net 2 "+5V"))
)
(footprint "DC:R1" (layer "F.Cu") (at 13.97 8.89)
(attr smd)
(fp_text reference "R1" (at 0 -1.725) (layer "F.SilkS"))
(fp_text value "10k_1%" (at 0 1.825) (layer "F.Fab"))
(pad "1" smd rect (at -1.016 0) (size 1.2 1.4)  (layers "F.Cu" "F.Mask") (net 3 "BUTTON_N"))
(pad "2" smd rect (at 1.016 0) (size 1.2 1.4)  (layers "F.Cu" "F.Mask") (net 1 "+3V3"))
)
(footprint "DC:R2" (layer "F.Cu") (at 16.51 15.24)
(attr smd)
(fp_text reference "R2" (at 0 -1.725) (layer "F.SilkS"))
(fp_text value "10k_1%" (at 0 1.825) (layer "F.Fab"))
(pad "1" smd rect (at -1.016 0) (size 1.2 1.4)  (layers "F.Cu" "F.Mask") (net 11 "LCD_CS"))
(pad "2" smd rect (at 1.016 0) (size 1.2 1.4)  (layers "F.Cu" "F.Mask") (net 1 "+3V3"))
)
(footprint "DC:R3" (layer "F.Cu") (at 16.51 20.32)
(attr smd)
(fp_text reference "R3" (at 0 -1.725) (layer "F.SilkS"))
(fp_text value "10k_1%" (at 0 1.825) (layer "F.Fab"))
(pad "1" smd rect (at -1.016 0) (size 1.2 1.4)  (layers "F.Cu" "F.Mask") (net 13 "LCD_RST"))
(pad "2" smd rect (at 1.016 0) (size 1.2 1.4)  (layers "F.Cu" "F.Mask") (net 1 "+3V3"))
)
(footprint "DC:R4" (layer "F.Cu") (at 11.43 38.1)
(attr smd)
(fp_text reference "R4" (at 0 -1.725) (layer "F.SilkS"))
(fp_text value "3.57k_1%" (at 0 1.825) (layer "F.Fab"))
(pad "1" smd rect (at -1.016 0) (size 1.2 1.4)  (layers "F.Cu" "F.Mask") (net 9 "ISET"))
(pad "2" smd rect (at 1.016 0) (size 1.2 1.4)  (layers "F.Cu" "F.Mask") (net 5 "GND"))
)
(footprint "DC:C1" (layer "F.Cu") (at 21.59 30.48)
(attr smd)
(fp_text reference "C1" (at 0 -1.9000000000000001) (layer "F.SilkS"))
(fp_text value "47uF_10V_X5R" (at 0 2.0) (layer "F.Fab"))
(pad "1" smd rect (at -1.524 0) (size 1.5 1.8)  (layers "F.Cu" "F.Mask") (net 2 "+5V"))
(pad "2" smd rect (at 1.524 0) (size 1.5 1.8)  (layers "F.Cu" "F.Mask") (net 5 "GND"))
)
(footprint "DC:C2" (layer "F.Cu") (at 39.37 10.16)
(attr smd)
(fp_text reference "C2" (at 0 -1.725) (layer "F.SilkS"))
(fp_text value "100nF_16V_X7R" (at 0 1.825) (layer "F.Fab"))
(pad "1" smd rect (at -1.016 0) (size 1.2 1.4)  (layers "F.Cu" "F.Mask") (net 4 "COMPUTE_5V"))
(pad "2" smd rect (at 1.016 0) (size 1.2 1.4)  (layers "F.Cu" "F.Mask") (net 5 "GND"))
)
(footprint "DC:C3" (layer "F.Cu") (at 39.37 15.24)
(attr smd)
(fp_text reference "C3" (at 0 -1.725) (layer "F.SilkS"))
(fp_text value "10uF_10V_X5R" (at 0 1.825) (layer "F.Fab"))
(pad "1" smd rect (at -1.016 0) (size 1.2 1.4)  (layers "F.Cu" "F.Mask") (net 1 "+3V3"))
(pad "2" smd rect (at 1.016 0) (size 1.2 1.4)  (layers "F.Cu" "F.Mask") (net 5 "GND"))
)
(footprint "DC:C4" (layer "F.Cu") (at 10.16 8.89)
(attr smd)
(fp_text reference "C4" (at 0 -1.725) (layer "F.SilkS"))
(fp_text value "100nF_16V_X7R" (at 0 1.825) (layer "F.Fab"))
(pad "1" smd rect (at -1.016 0) (size 1.2 1.4)  (layers "F.Cu" "F.Mask") (net 3 "BUTTON_N"))
(pad "2" smd rect (at 1.016 0) (size 1.2 1.4)  (layers "F.Cu" "F.Mask") (net 5 "GND"))
)
(footprint "DC:C5" (layer "F.Cu") (at 16.51 25.4)
(attr smd)
(fp_text reference "C5" (at 0 -1.9000000000000001) (layer "F.SilkS"))
(fp_text value "47uF_10V_X5R" (at 0 2.0) (layer "F.Fab"))
(pad "1" smd rect (at -1.524 0) (size 1.5 1.8)  (layers "F.Cu" "F.Mask") (net 19 "SYS_SW"))
(pad "2" smd rect (at 1.524 0) (size 1.5 1.8)  (layers "F.Cu" "F.Mask") (net 5 "GND"))
)
(footprint "DC:M2_CLEARANCE" (layer "F.Cu") (at 4 4) (attr board_only exclude_from_pos_files exclude_from_bom) (fp_text reference "H1" (at 0 0) (layer "F.Fab")) (pad "" np_thru_hole circle (at 0 0) (size 2.5 2.5) (drill 2.5) (layers "*.Cu" "*.Mask")))
(footprint "DC:M2_CLEARANCE" (layer "F.Cu") (at 50 4) (attr board_only exclude_from_pos_files exclude_from_bom) (fp_text reference "H2" (at 0 0) (layer "F.Fab")) (pad "" np_thru_hole circle (at 0 0) (size 2.5 2.5) (drill 2.5) (layers "*.Cu" "*.Mask")))
(footprint "DC:M2_CLEARANCE" (layer "F.Cu") (at 4 42) (attr board_only exclude_from_pos_files exclude_from_bom) (fp_text reference "H3" (at 0 0) (layer "F.Fab")) (pad "" np_thru_hole circle (at 0 0) (size 2.5 2.5) (drill 2.5) (layers "*.Cu" "*.Mask")))
(footprint "DC:M2_CLEARANCE" (layer "F.Cu") (at 50 42) (attr board_only exclude_from_pos_files exclude_from_bom) (fp_text reference "H4" (at 0 0) (layer "F.Fab")) (pad "" np_thru_hole circle (at 0 0) (size 2.5 2.5) (drill 2.5) (layers "*.Cu" "*.Mask")))
(gr_line (start 0 0) (end 54 0) (layer "Edge.Cuts"))
(gr_line (start 54 0) (end 54 46) (layer "Edge.Cuts"))
(gr_line (start 54 46) (end 0 46) (layer "Edge.Cuts"))
(gr_line (start 0 46) (end 0 0) (layer "Edge.Cuts"))
(gr_text "DC-E02 CANDIDATE" (at 27 36) (layer "F.SilkS"))
)
