(kicad_sch (version 20230121) (generator desktop_companion) (paper "A3")
(title_block (title "DC-E02 Desktop companion carrier") (rev "E02") (comment 1 "ENGINEERING CANDIDATE; NATIVE ERC/DRC AND BENCH QUALIFICATION OPEN"))
(lib_symbols
(symbol "DC:U1" (pin_names (offset 0.6)) (in_bom yes) (on_board yes)
(property "Reference" "U" (at 0 19.78 0))
(property "Value" "Seeed_XIAO_ESP32S3_nonSense" (at 0 21.78 0))
(symbol "U1_0_1" (rectangle (start 0 17.78) (end 26 -17.78) (fill (type background))))
(symbol "U1_1_1"
(pin bidirectional line (at -2.54 16.51 0) (length 2.54) (name "D0_GPIO1") (number "1"))
(pin bidirectional line (at -2.54 13.97 0) (length 2.54) (name "D1_GPIO2") (number "2"))
(pin bidirectional line (at -2.54 11.430000000000001 0) (length 2.54) (name "D2_GPIO3_STRAP") (number "3"))
(pin bidirectional line (at -2.54 8.89 0) (length 2.54) (name "D3_GPIO4") (number "4"))
(pin bidirectional line (at -2.54 6.350000000000001 0) (length 2.54) (name "D4_GPIO5") (number "5"))
(pin bidirectional line (at -2.54 3.8100000000000005 0) (length 2.54) (name "D5_GPIO6") (number "6"))
(pin bidirectional line (at -2.54 1.2699999999999996 0) (length 2.54) (name "D6_GPIO43") (number "7"))
(pin bidirectional line (at -2.54 -1.2699999999999996 0) (length 2.54) (name "D7_GPIO44") (number "8"))
(pin bidirectional line (at -2.54 -3.8099999999999987 0) (length 2.54) (name "D8_GPIO7") (number "9"))
(pin bidirectional line (at -2.54 -6.349999999999998 0) (length 2.54) (name "D9_GPIO8") (number "10"))
(pin bidirectional line (at -2.54 -8.89 0) (length 2.54) (name "D10_GPIO9") (number "11"))
(pin power_out line (at -2.54 -11.43 0) (length 2.54) (name "3V3_OUT") (number "12"))
(pin power_in line (at -2.54 -13.969999999999999 0) (length 2.54) (name "GND") (number "13"))
(pin power_in line (at -2.54 -16.509999999999998 0) (length 2.54) (name "VBUS_IN") (number "14"))
))
(symbol "DC:J1" (pin_names (offset 0.6)) (in_bom yes) (on_board yes)
(property "Reference" "J" (at 0 7.08 0))
(property "Value" "BQ24074_OUT" (at 0 9.08 0))
(symbol "J1_0_1" (rectangle (start 0 5.08) (end 26 -5.08) (fill (type background))))
(symbol "J1_1_1"
(pin passive line (at -2.54 3.81 0) (length 2.54) (name "SYS_RAW") (number "1"))
(pin passive line (at -2.54 1.27 0) (length 2.54) (name "GND") (number "2"))
))
(symbol "DC:J2" (pin_names (offset 0.6)) (in_bom yes) (on_board yes)
(property "Reference" "J" (at 0 12.16 0))
(property "Value" "DISPLAY_5206" (at 0 14.16 0))
(symbol "J2_0_1" (rectangle (start 0 10.16) (end 26 -10.16) (fill (type background))))
(symbol "J2_1_1"
(pin passive line (at -2.54 8.89 0) (length 2.54) (name "+3V3") (number "1"))
(pin passive line (at -2.54 6.35 0) (length 2.54) (name "GND") (number "2"))
(pin passive line (at -2.54 3.8100000000000005 0) (length 2.54) (name "SPI_SCK") (number "3"))
(pin passive line (at -2.54 1.2699999999999996 0) (length 2.54) (name "SPI_MOSI") (number "4"))
(pin passive line (at -2.54 -1.2699999999999996 0) (length 2.54) (name "LCD_CS") (number "5"))
(pin passive line (at -2.54 -3.8100000000000005 0) (length 2.54) (name "LCD_DC") (number "6"))
(pin passive line (at -2.54 -6.350000000000001 0) (length 2.54) (name "LCD_RST") (number "7"))
(pin passive line (at -2.54 -8.89 0) (length 2.54) (name "LCD_BL") (number "8"))
))
(symbol "DC:J3" (pin_names (offset 0.6)) (in_bom yes) (on_board yes)
(property "Reference" "J" (at 0 8.35 0))
(property "Value" "I2S_AUDIO_OPTION" (at 0 10.35 0))
(symbol "J3_0_1" (rectangle (start 0 6.35) (end 26 -6.35) (fill (type background))))
(symbol "J3_1_1"
(pin passive line (at -2.54 5.08 0) (length 2.54) (name "+5V") (number "1"))
(pin passive line (at -2.54 2.5399999999999996 0) (length 2.54) (name "GND") (number "2"))
(pin passive line (at -2.54 0.0 0) (length 2.54) (name "I2S_BCLK") (number "3"))
(pin passive line (at -2.54 -2.540000000000001 0) (length 2.54) (name "I2S_LRCLK") (number "4"))
(pin passive line (at -2.54 -5.08 0) (length 2.54) (name "I2S_DIN") (number "5"))
))
(symbol "DC:J4" (pin_names (offset 0.6)) (in_bom yes) (on_board yes)
(property "Reference" "J" (at 0 7.08 0))
(property "Value" "POWER_SWITCH" (at 0 9.08 0))
(symbol "J4_0_1" (rectangle (start 0 5.08) (end 26 -5.08) (fill (type background))))
(symbol "J4_1_1"
(pin passive line (at -2.54 3.81 0) (length 2.54) (name "SYS_FUSED") (number "1"))
(pin passive line (at -2.54 1.27 0) (length 2.54) (name "SYS_SW") (number "2"))
))
(symbol "DC:J5" (pin_names (offset 0.6)) (in_bom yes) (on_board yes)
(property "Reference" "J" (at 0 7.08 0))
(property "Value" "S7V8F5_WIRED" (at 0 9.08 0))
(symbol "J5_0_1" (rectangle (start 0 5.08) (end 26 -5.08) (fill (type background))))
(symbol "J5_1_1"
(pin passive line (at -2.54 3.81 0) (length 2.54) (name "SYS_SW") (number "1"))
(pin passive line (at -2.54 1.27 0) (length 2.54) (name "GND") (number "2"))
(pin passive line (at -2.54 -1.2699999999999996 0) (length 2.54) (name "+5V") (number "3"))
))
(symbol "DC:J6" (pin_names (offset 0.6)) (in_bom yes) (on_board yes)
(property "Reference" "J" (at 0 7.08 0))
(property "Value" "MOMENTARY_BUTTON" (at 0 9.08 0))
(symbol "J6_0_1" (rectangle (start 0 5.08) (end 26 -5.08) (fill (type background))))
(symbol "J6_1_1"
(pin passive line (at -2.54 3.81 0) (length 2.54) (name "BUTTON_N") (number "1"))
(pin passive line (at -2.54 1.27 0) (length 2.54) (name "GND") (number "2"))
))
(symbol "DC:J7" (pin_names (offset 0.6)) (in_bom yes) (on_board yes)
(property "Reference" "J" (at 0 7.08 0))
(property "Value" "CHARGER_PROGRAM_NTC" (at 0 9.08 0))
(symbol "J7_0_1" (rectangle (start 0 5.08) (end 26 -5.08) (fill (type background))))
(symbol "J7_1_1"
(pin passive line (at -2.54 3.81 0) (length 2.54) (name "ISET") (number "1"))
(pin passive line (at -2.54 1.27 0) (length 2.54) (name "GND") (number "2"))
(pin passive line (at -2.54 -1.2699999999999996 0) (length 2.54) (name "NTC_TS") (number "3"))
))
(symbol "DC:J8" (pin_names (offset 0.6)) (in_bom yes) (on_board yes)
(property "Reference" "J" (at 0 7.08 0))
(property "Value" "103AT2_PACK_SENSOR" (at 0 9.08 0))
(symbol "J8_0_1" (rectangle (start 0 5.08) (end 26 -5.08) (fill (type background))))
(symbol "J8_1_1"
(pin passive line (at -2.54 3.81 0) (length 2.54) (name "NTC_TS") (number "1"))
(pin passive line (at -2.54 1.27 0) (length 2.54) (name "GND") (number "2"))
))
(symbol "DC:F1" (pin_names (offset 0.6)) (in_bom yes) (on_board yes)
(property "Reference" "F" (at 0 7.08 0))
(property "Value" "MF-MSMF110_16X-2" (at 0 9.08 0))
(symbol "F1_0_1" (rectangle (start 0 5.08) (end 26 -5.08) (fill (type background))))
(symbol "F1_1_1"
(pin passive line (at -2.54 3.81 0) (length 2.54) (name "SYS_RAW") (number "1"))
(pin passive line (at -2.54 1.27 0) (length 2.54) (name "SYS_FUSED") (number "2"))
))
(symbol "DC:D1" (pin_names (offset 0.6)) (in_bom yes) (on_board yes)
(property "Reference" "D" (at 0 7.08 0))
(property "Value" "SS14_SCHOTTKY" (at 0 9.08 0))
(symbol "D1_0_1" (rectangle (start 0 5.08) (end 26 -5.08) (fill (type background))))
(symbol "D1_1_1"
(pin passive line (at -2.54 3.81 0) (length 2.54) (name "K") (number "1"))
(pin passive line (at -2.54 1.27 0) (length 2.54) (name "A") (number "2"))
))
(symbol "DC:R1" (pin_names (offset 0.6)) (in_bom yes) (on_board yes)
(property "Reference" "R" (at 0 7.08 0))
(property "Value" "10k_1%" (at 0 9.08 0))
(symbol "R1_0_1" (rectangle (start 0 5.08) (end 26 -5.08) (fill (type background))))
(symbol "R1_1_1"
(pin passive line (at -2.54 3.81 0) (length 2.54) (name "BUTTON_N") (number "1"))
(pin passive line (at -2.54 1.27 0) (length 2.54) (name "+3V3") (number "2"))
))
(symbol "DC:R2" (pin_names (offset 0.6)) (in_bom yes) (on_board yes)
(property "Reference" "R" (at 0 7.08 0))
(property "Value" "10k_1%" (at 0 9.08 0))
(symbol "R2_0_1" (rectangle (start 0 5.08) (end 26 -5.08) (fill (type background))))
(symbol "R2_1_1"
(pin passive line (at -2.54 3.81 0) (length 2.54) (name "LCD_CS") (number "1"))
(pin passive line (at -2.54 1.27 0) (length 2.54) (name "+3V3") (number "2"))
))
(symbol "DC:R3" (pin_names (offset 0.6)) (in_bom yes) (on_board yes)
(property "Reference" "R" (at 0 7.08 0))
(property "Value" "10k_1%" (at 0 9.08 0))
(symbol "R3_0_1" (rectangle (start 0 5.08) (end 26 -5.08) (fill (type background))))
(symbol "R3_1_1"
(pin passive line (at -2.54 3.81 0) (length 2.54) (name "LCD_RST") (number "1"))
(pin passive line (at -2.54 1.27 0) (length 2.54) (name "+3V3") (number "2"))
))
(symbol "DC:R4" (pin_names (offset 0.6)) (in_bom yes) (on_board yes)
(property "Reference" "R" (at 0 7.08 0))
(property "Value" "3.57k_1%" (at 0 9.08 0))
(symbol "R4_0_1" (rectangle (start 0 5.08) (end 26 -5.08) (fill (type background))))
(symbol "R4_1_1"
(pin passive line (at -2.54 3.81 0) (length 2.54) (name "ISET") (number "1"))
(pin passive line (at -2.54 1.27 0) (length 2.54) (name "GND") (number "2"))
))
(symbol "DC:C1" (pin_names (offset 0.6)) (in_bom yes) (on_board yes)
(property "Reference" "C" (at 0 7.08 0))
(property "Value" "47uF_10V_X5R" (at 0 9.08 0))
(symbol "C1_0_1" (rectangle (start 0 5.08) (end 26 -5.08) (fill (type background))))
(symbol "C1_1_1"
(pin passive line (at -2.54 3.81 0) (length 2.54) (name "+5V") (number "1"))
(pin passive line (at -2.54 1.27 0) (length 2.54) (name "GND") (number "2"))
))
(symbol "DC:C2" (pin_names (offset 0.6)) (in_bom yes) (on_board yes)
(property "Reference" "C" (at 0 7.08 0))
(property "Value" "100nF_16V_X7R" (at 0 9.08 0))
(symbol "C2_0_1" (rectangle (start 0 5.08) (end 26 -5.08) (fill (type background))))
(symbol "C2_1_1"
(pin passive line (at -2.54 3.81 0) (length 2.54) (name "COMPUTE_5V") (number "1"))
(pin passive line (at -2.54 1.27 0) (length 2.54) (name "GND") (number "2"))
))
(symbol "DC:C3" (pin_names (offset 0.6)) (in_bom yes) (on_board yes)
(property "Reference" "C" (at 0 7.08 0))
(property "Value" "10uF_10V_X5R" (at 0 9.08 0))
(symbol "C3_0_1" (rectangle (start 0 5.08) (end 26 -5.08) (fill (type background))))
(symbol "C3_1_1"
(pin passive line (at -2.54 3.81 0) (length 2.54) (name "+3V3") (number "1"))
(pin passive line (at -2.54 1.27 0) (length 2.54) (name "GND") (number "2"))
))
(symbol "DC:C4" (pin_names (offset 0.6)) (in_bom yes) (on_board yes)
(property "Reference" "C" (at 0 7.08 0))
(property "Value" "100nF_16V_X7R" (at 0 9.08 0))
(symbol "C4_0_1" (rectangle (start 0 5.08) (end 26 -5.08) (fill (type background))))
(symbol "C4_1_1"
(pin passive line (at -2.54 3.81 0) (length 2.54) (name "BUTTON_N") (number "1"))
(pin passive line (at -2.54 1.27 0) (length 2.54) (name "GND") (number "2"))
))
(symbol "DC:C5" (pin_names (offset 0.6)) (in_bom yes) (on_board yes)
(property "Reference" "C" (at 0 7.08 0))
(property "Value" "47uF_10V_X5R" (at 0 9.08 0))
(symbol "C5_0_1" (rectangle (start 0 5.08) (end 26 -5.08) (fill (type background))))
(symbol "C5_1_1"
(pin passive line (at -2.54 3.81 0) (length 2.54) (name "SYS_SW") (number "1"))
(pin passive line (at -2.54 1.27 0) (length 2.54) (name "GND") (number "2"))
))
(symbol "DC:PWR_FLAG" (pin_names (offset 0)) (in_bom no) (on_board no) (property "Reference" "#FLG" (at 0 2.54 0)) (property "Value" "PWR_FLAG" (at 0 5.08 0)) (symbol "PWR_FLAG_1_1" (pin power_out line (at 0 0 90) (length 0) (name "pwr") (number "1"))))
)
(symbol (lib_id "DC:U1") (at 38.1 35.56 0) (unit 1) (in_bom yes) (on_board yes)
(property "Reference" "U1" (at 51.1 14.780000000000001 0))
(property "Value" "Seeed_XIAO_ESP32S3_nonSense" (at 51.1 56.34 0))
(property "Footprint" "DC:U1" (at 38.1 35.56 0))
(instances (project "desktop-companion" (path (reference "U1") (unit 1))))
)
(wire (pts (xy 30.480000000000004 19.05) (xy 35.56 19.05)))
(global_label "LCD_CS" (shape bidirectional) (at 30.480000000000004 19.05 0))
(wire (pts (xy 30.480000000000004 21.590000000000003) (xy 35.56 21.590000000000003)))
(global_label "LCD_DC" (shape bidirectional) (at 30.480000000000004 21.590000000000003 0))
(no_connect (at 35.56 24.130000000000003))
(wire (pts (xy 30.480000000000004 26.67) (xy 35.56 26.67)))
(global_label "LCD_RST" (shape bidirectional) (at 30.480000000000004 26.67 0))
(wire (pts (xy 30.480000000000004 29.21) (xy 35.56 29.21)))
(global_label "LCD_BL" (shape bidirectional) (at 30.480000000000004 29.21 0))
(wire (pts (xy 30.480000000000004 31.75) (xy 35.56 31.75)))
(global_label "BUTTON_N" (shape bidirectional) (at 30.480000000000004 31.75 0))
(wire (pts (xy 30.480000000000004 34.290000000000006) (xy 35.56 34.290000000000006)))
(global_label "I2S_BCLK" (shape bidirectional) (at 30.480000000000004 34.290000000000006 0))
(wire (pts (xy 30.480000000000004 36.83) (xy 35.56 36.83)))
(global_label "I2S_LRCLK" (shape bidirectional) (at 30.480000000000004 36.83 0))
(wire (pts (xy 30.480000000000004 39.370000000000005) (xy 35.56 39.370000000000005)))
(global_label "SPI_SCK" (shape bidirectional) (at 30.480000000000004 39.370000000000005 0))
(wire (pts (xy 30.480000000000004 41.91) (xy 35.56 41.91)))
(global_label "I2S_DIN" (shape bidirectional) (at 30.480000000000004 41.91 0))
(wire (pts (xy 30.480000000000004 44.45) (xy 35.56 44.45)))
(global_label "SPI_MOSI" (shape bidirectional) (at 30.480000000000004 44.45 0))
(wire (pts (xy 30.480000000000004 46.99) (xy 35.56 46.99)))
(global_label "+3V3" (shape bidirectional) (at 30.480000000000004 46.99 0))
(wire (pts (xy 30.480000000000004 49.53) (xy 35.56 49.53)))
(global_label "GND" (shape bidirectional) (at 30.480000000000004 49.53 0))
(wire (pts (xy 30.480000000000004 52.07) (xy 35.56 52.07)))
(global_label "COMPUTE_5V" (shape bidirectional) (at 30.480000000000004 52.07 0))
(symbol (lib_id "DC:J1") (at 114.30000000000001 35.56 0) (unit 1) (in_bom yes) (on_board yes)
(property "Reference" "J1" (at 127.30000000000001 27.480000000000004 0))
(property "Value" "BQ24074_OUT" (at 127.30000000000001 43.64 0))
(property "Footprint" "DC:J1" (at 114.30000000000001 35.56 0))
(instances (project "desktop-companion" (path (reference "J1") (unit 1))))
)
(wire (pts (xy 106.68 31.750000000000004) (xy 111.76 31.750000000000004)))
(global_label "SYS_RAW" (shape bidirectional) (at 106.68 31.750000000000004 0))
(wire (pts (xy 106.68 34.29) (xy 111.76 34.29)))
(global_label "GND" (shape bidirectional) (at 106.68 34.29 0))
(symbol (lib_id "DC:J2") (at 190.5 35.56 0) (unit 1) (in_bom yes) (on_board yes)
(property "Reference" "J2" (at 203.5 22.400000000000002 0))
(property "Value" "DISPLAY_5206" (at 203.5 48.72 0))
(property "Footprint" "DC:J2" (at 190.5 35.56 0))
(instances (project "desktop-companion" (path (reference "J2") (unit 1))))
)
(wire (pts (xy 182.88 26.67) (xy 187.96 26.67)))
(global_label "+3V3" (shape bidirectional) (at 182.88 26.67 0))
(wire (pts (xy 182.88 29.21) (xy 187.96 29.21)))
(global_label "GND" (shape bidirectional) (at 182.88 29.21 0))
(wire (pts (xy 182.88 31.75) (xy 187.96 31.75)))
(global_label "SPI_SCK" (shape bidirectional) (at 182.88 31.75 0))
(wire (pts (xy 182.88 34.290000000000006) (xy 187.96 34.290000000000006)))
(global_label "SPI_MOSI" (shape bidirectional) (at 182.88 34.290000000000006 0))
(wire (pts (xy 182.88 36.83) (xy 187.96 36.83)))
(global_label "LCD_CS" (shape bidirectional) (at 182.88 36.83 0))
(wire (pts (xy 182.88 39.370000000000005) (xy 187.96 39.370000000000005)))
(global_label "LCD_DC" (shape bidirectional) (at 182.88 39.370000000000005 0))
(wire (pts (xy 182.88 41.910000000000004) (xy 187.96 41.910000000000004)))
(global_label "LCD_RST" (shape bidirectional) (at 182.88 41.910000000000004 0))
(wire (pts (xy 182.88 44.45) (xy 187.96 44.45)))
(global_label "LCD_BL" (shape bidirectional) (at 182.88 44.45 0))
(symbol (lib_id "DC:J3") (at 266.70000000000005 35.56 0) (unit 1) (in_bom yes) (on_board yes)
(property "Reference" "J3" (at 279.70000000000005 26.21 0))
(property "Value" "I2S_AUDIO_OPTION" (at 279.70000000000005 44.910000000000004 0))
(property "Footprint" "DC:J3" (at 266.70000000000005 35.56 0))
(instances (project "desktop-companion" (path (reference "J3") (unit 1))))
)
(wire (pts (xy 259.08000000000004 30.480000000000004) (xy 264.16 30.480000000000004)))
(global_label "+5V" (shape bidirectional) (at 259.08000000000004 30.480000000000004 0))
(wire (pts (xy 259.08000000000004 33.02) (xy 264.16 33.02)))
(global_label "GND" (shape bidirectional) (at 259.08000000000004 33.02 0))
(wire (pts (xy 259.08000000000004 35.56) (xy 264.16 35.56)))
(global_label "I2S_BCLK" (shape bidirectional) (at 259.08000000000004 35.56 0))
(wire (pts (xy 259.08000000000004 38.1) (xy 264.16 38.1)))
(global_label "I2S_LRCLK" (shape bidirectional) (at 259.08000000000004 38.1 0))
(wire (pts (xy 259.08000000000004 40.64) (xy 264.16 40.64)))
(global_label "I2S_DIN" (shape bidirectional) (at 259.08000000000004 40.64 0))
(symbol (lib_id "DC:J4") (at 342.90000000000003 35.56 0) (unit 1) (in_bom yes) (on_board yes)
(property "Reference" "J4" (at 355.90000000000003 27.480000000000004 0))
(property "Value" "POWER_SWITCH" (at 355.90000000000003 43.64 0))
(property "Footprint" "DC:J4" (at 342.90000000000003 35.56 0))
(instances (project "desktop-companion" (path (reference "J4") (unit 1))))
)
(wire (pts (xy 335.28000000000003 31.750000000000004) (xy 340.36 31.750000000000004)))
(global_label "SYS_FUSED" (shape bidirectional) (at 335.28000000000003 31.750000000000004 0))
(wire (pts (xy 335.28000000000003 34.29) (xy 340.36 34.29)))
(global_label "SYS_SW" (shape bidirectional) (at 335.28000000000003 34.29 0))
(symbol (lib_id "DC:J5") (at 38.1 91.44 0) (unit 1) (in_bom yes) (on_board yes)
(property "Reference" "J5" (at 51.1 83.36 0))
(property "Value" "S7V8F5_WIRED" (at 51.1 99.52 0))
(property "Footprint" "DC:J5" (at 38.1 91.44 0))
(instances (project "desktop-companion" (path (reference "J5") (unit 1))))
)
(wire (pts (xy 30.480000000000004 87.63) (xy 35.56 87.63)))
(global_label "SYS_SW" (shape bidirectional) (at 30.480000000000004 87.63 0))
(wire (pts (xy 30.480000000000004 90.17) (xy 35.56 90.17)))
(global_label "GND" (shape bidirectional) (at 30.480000000000004 90.17 0))
(wire (pts (xy 30.480000000000004 92.71) (xy 35.56 92.71)))
(global_label "+5V" (shape bidirectional) (at 30.480000000000004 92.71 0))
(symbol (lib_id "DC:J6") (at 114.30000000000001 91.44 0) (unit 1) (in_bom yes) (on_board yes)
(property "Reference" "J6" (at 127.30000000000001 83.36 0))
(property "Value" "MOMENTARY_BUTTON" (at 127.30000000000001 99.52 0))
(property "Footprint" "DC:J6" (at 114.30000000000001 91.44 0))
(instances (project "desktop-companion" (path (reference "J6") (unit 1))))
)
(wire (pts (xy 106.68 87.63) (xy 111.76 87.63)))
(global_label "BUTTON_N" (shape bidirectional) (at 106.68 87.63 0))
(wire (pts (xy 106.68 90.17) (xy 111.76 90.17)))
(global_label "GND" (shape bidirectional) (at 106.68 90.17 0))
(symbol (lib_id "DC:J7") (at 190.5 91.44 0) (unit 1) (in_bom yes) (on_board yes)
(property "Reference" "J7" (at 203.5 83.36 0))
(property "Value" "CHARGER_PROGRAM_NTC" (at 203.5 99.52 0))
(property "Footprint" "DC:J7" (at 190.5 91.44 0))
(instances (project "desktop-companion" (path (reference "J7") (unit 1))))
)
(wire (pts (xy 182.88 87.63) (xy 187.96 87.63)))
(global_label "ISET" (shape bidirectional) (at 182.88 87.63 0))
(wire (pts (xy 182.88 90.17) (xy 187.96 90.17)))
(global_label "GND" (shape bidirectional) (at 182.88 90.17 0))
(wire (pts (xy 182.88 92.71) (xy 187.96 92.71)))
(global_label "NTC_TS" (shape bidirectional) (at 182.88 92.71 0))
(symbol (lib_id "DC:J8") (at 266.70000000000005 91.44 0) (unit 1) (in_bom yes) (on_board yes)
(property "Reference" "J8" (at 279.70000000000005 83.36 0))
(property "Value" "103AT2_PACK_SENSOR" (at 279.70000000000005 99.52 0))
(property "Footprint" "DC:J8" (at 266.70000000000005 91.44 0))
(instances (project "desktop-companion" (path (reference "J8") (unit 1))))
)
(wire (pts (xy 259.08000000000004 87.63) (xy 264.16 87.63)))
(global_label "NTC_TS" (shape bidirectional) (at 259.08000000000004 87.63 0))
(wire (pts (xy 259.08000000000004 90.17) (xy 264.16 90.17)))
(global_label "GND" (shape bidirectional) (at 259.08000000000004 90.17 0))
(symbol (lib_id "DC:F1") (at 342.90000000000003 91.44 0) (unit 1) (in_bom yes) (on_board yes)
(property "Reference" "F1" (at 355.90000000000003 83.36 0))
(property "Value" "MF-MSMF110_16X-2" (at 355.90000000000003 99.52 0))
(property "Footprint" "DC:F1" (at 342.90000000000003 91.44 0))
(instances (project "desktop-companion" (path (reference "F1") (unit 1))))
)
(wire (pts (xy 335.28000000000003 87.63) (xy 340.36 87.63)))
(global_label "SYS_RAW" (shape bidirectional) (at 335.28000000000003 87.63 0))
(wire (pts (xy 335.28000000000003 90.17) (xy 340.36 90.17)))
(global_label "SYS_FUSED" (shape bidirectional) (at 335.28000000000003 90.17 0))
(symbol (lib_id "DC:D1") (at 38.1 147.32 0) (unit 1) (in_bom yes) (on_board yes)
(property "Reference" "D1" (at 51.1 139.23999999999998 0))
(property "Value" "SS14_SCHOTTKY" (at 51.1 155.4 0))
(property "Footprint" "DC:D1" (at 38.1 147.32 0))
(instances (project "desktop-companion" (path (reference "D1") (unit 1))))
)
(wire (pts (xy 30.480000000000004 143.51) (xy 35.56 143.51)))
(global_label "COMPUTE_5V" (shape bidirectional) (at 30.480000000000004 143.51 0))
(wire (pts (xy 30.480000000000004 146.04999999999998) (xy 35.56 146.04999999999998)))
(global_label "+5V" (shape bidirectional) (at 30.480000000000004 146.04999999999998 0))
(symbol (lib_id "DC:R1") (at 114.30000000000001 147.32 0) (unit 1) (in_bom yes) (on_board yes)
(property "Reference" "R1" (at 127.30000000000001 139.23999999999998 0))
(property "Value" "10k_1%" (at 127.30000000000001 155.4 0))
(property "Footprint" "DC:R1" (at 114.30000000000001 147.32 0))
(instances (project "desktop-companion" (path (reference "R1") (unit 1))))
)
(wire (pts (xy 106.68 143.51) (xy 111.76 143.51)))
(global_label "BUTTON_N" (shape bidirectional) (at 106.68 143.51 0))
(wire (pts (xy 106.68 146.04999999999998) (xy 111.76 146.04999999999998)))
(global_label "+3V3" (shape bidirectional) (at 106.68 146.04999999999998 0))
(symbol (lib_id "DC:R2") (at 190.5 147.32 0) (unit 1) (in_bom yes) (on_board yes)
(property "Reference" "R2" (at 203.5 139.23999999999998 0))
(property "Value" "10k_1%" (at 203.5 155.4 0))
(property "Footprint" "DC:R2" (at 190.5 147.32 0))
(instances (project "desktop-companion" (path (reference "R2") (unit 1))))
)
(wire (pts (xy 182.88 143.51) (xy 187.96 143.51)))
(global_label "LCD_CS" (shape bidirectional) (at 182.88 143.51 0))
(wire (pts (xy 182.88 146.04999999999998) (xy 187.96 146.04999999999998)))
(global_label "+3V3" (shape bidirectional) (at 182.88 146.04999999999998 0))
(symbol (lib_id "DC:R3") (at 266.70000000000005 147.32 0) (unit 1) (in_bom yes) (on_board yes)
(property "Reference" "R3" (at 279.70000000000005 139.23999999999998 0))
(property "Value" "10k_1%" (at 279.70000000000005 155.4 0))
(property "Footprint" "DC:R3" (at 266.70000000000005 147.32 0))
(instances (project "desktop-companion" (path (reference "R3") (unit 1))))
)
(wire (pts (xy 259.08000000000004 143.51) (xy 264.16 143.51)))
(global_label "LCD_RST" (shape bidirectional) (at 259.08000000000004 143.51 0))
(wire (pts (xy 259.08000000000004 146.04999999999998) (xy 264.16 146.04999999999998)))
(global_label "+3V3" (shape bidirectional) (at 259.08000000000004 146.04999999999998 0))
(symbol (lib_id "DC:R4") (at 342.90000000000003 147.32 0) (unit 1) (in_bom yes) (on_board yes)
(property "Reference" "R4" (at 355.90000000000003 139.23999999999998 0))
(property "Value" "3.57k_1%" (at 355.90000000000003 155.4 0))
(property "Footprint" "DC:R4" (at 342.90000000000003 147.32 0))
(instances (project "desktop-companion" (path (reference "R4") (unit 1))))
)
(wire (pts (xy 335.28000000000003 143.51) (xy 340.36 143.51)))
(global_label "ISET" (shape bidirectional) (at 335.28000000000003 143.51 0))
(wire (pts (xy 335.28000000000003 146.04999999999998) (xy 340.36 146.04999999999998)))
(global_label "GND" (shape bidirectional) (at 335.28000000000003 146.04999999999998 0))
(symbol (lib_id "DC:C1") (at 38.1 203.20000000000002 0) (unit 1) (in_bom yes) (on_board yes)
(property "Reference" "C1" (at 51.1 195.12 0))
(property "Value" "47uF_10V_X5R" (at 51.1 211.28000000000003 0))
(property "Footprint" "DC:C1" (at 38.1 203.20000000000002 0))
(instances (project "desktop-companion" (path (reference "C1") (unit 1))))
)
(wire (pts (xy 30.480000000000004 199.39000000000001) (xy 35.56 199.39000000000001)))
(global_label "+5V" (shape bidirectional) (at 30.480000000000004 199.39000000000001 0))
(wire (pts (xy 30.480000000000004 201.93) (xy 35.56 201.93)))
(global_label "GND" (shape bidirectional) (at 30.480000000000004 201.93 0))
(symbol (lib_id "DC:C2") (at 114.30000000000001 203.20000000000002 0) (unit 1) (in_bom yes) (on_board yes)
(property "Reference" "C2" (at 127.30000000000001 195.12 0))
(property "Value" "100nF_16V_X7R" (at 127.30000000000001 211.28000000000003 0))
(property "Footprint" "DC:C2" (at 114.30000000000001 203.20000000000002 0))
(instances (project "desktop-companion" (path (reference "C2") (unit 1))))
)
(wire (pts (xy 106.68 199.39000000000001) (xy 111.76 199.39000000000001)))
(global_label "COMPUTE_5V" (shape bidirectional) (at 106.68 199.39000000000001 0))
(wire (pts (xy 106.68 201.93) (xy 111.76 201.93)))
(global_label "GND" (shape bidirectional) (at 106.68 201.93 0))
(symbol (lib_id "DC:C3") (at 190.5 203.20000000000002 0) (unit 1) (in_bom yes) (on_board yes)
(property "Reference" "C3" (at 203.5 195.12 0))
(property "Value" "10uF_10V_X5R" (at 203.5 211.28000000000003 0))
(property "Footprint" "DC:C3" (at 190.5 203.20000000000002 0))
(instances (project "desktop-companion" (path (reference "C3") (unit 1))))
)
(wire (pts (xy 182.88 199.39000000000001) (xy 187.96 199.39000000000001)))
(global_label "+3V3" (shape bidirectional) (at 182.88 199.39000000000001 0))
(wire (pts (xy 182.88 201.93) (xy 187.96 201.93)))
(global_label "GND" (shape bidirectional) (at 182.88 201.93 0))
(symbol (lib_id "DC:C4") (at 266.70000000000005 203.20000000000002 0) (unit 1) (in_bom yes) (on_board yes)
(property "Reference" "C4" (at 279.70000000000005 195.12 0))
(property "Value" "100nF_16V_X7R" (at 279.70000000000005 211.28000000000003 0))
(property "Footprint" "DC:C4" (at 266.70000000000005 203.20000000000002 0))
(instances (project "desktop-companion" (path (reference "C4") (unit 1))))
)
(wire (pts (xy 259.08000000000004 199.39000000000001) (xy 264.16 199.39000000000001)))
(global_label "BUTTON_N" (shape bidirectional) (at 259.08000000000004 199.39000000000001 0))
(wire (pts (xy 259.08000000000004 201.93) (xy 264.16 201.93)))
(global_label "GND" (shape bidirectional) (at 259.08000000000004 201.93 0))
(symbol (lib_id "DC:C5") (at 342.90000000000003 203.20000000000002 0) (unit 1) (in_bom yes) (on_board yes)
(property "Reference" "C5" (at 355.90000000000003 195.12 0))
(property "Value" "47uF_10V_X5R" (at 355.90000000000003 211.28000000000003 0))
(property "Footprint" "DC:C5" (at 342.90000000000003 203.20000000000002 0))
(instances (project "desktop-companion" (path (reference "C5") (unit 1))))
)
(wire (pts (xy 335.28000000000003 199.39000000000001) (xy 340.36 199.39000000000001)))
(global_label "SYS_SW" (shape bidirectional) (at 335.28000000000003 199.39000000000001 0))
(wire (pts (xy 335.28000000000003 201.93) (xy 340.36 201.93)))
(global_label "GND" (shape bidirectional) (at 335.28000000000003 201.93 0))
(symbol (lib_id "DC:PWR_FLAG") (at 38.1 243.84 0) (unit 1) (in_bom no) (on_board no) (property "Reference" "#FLG01" (at 38.1 238.76 0)) (property "Value" "External power declaration" (at 38.1 241.3 0)) (instances (project "desktop-companion" (path (reference "#FLG01") (unit 1)))))
(global_label "GND" (shape bidirectional) (at 38.1 243.84 0))
(symbol (lib_id "DC:PWR_FLAG") (at 114.30000000000001 243.84 0) (unit 1) (in_bom no) (on_board no) (property "Reference" "#FLG02" (at 114.30000000000001 238.76 0)) (property "Value" "External power declaration" (at 114.30000000000001 241.3 0)) (instances (project "desktop-companion" (path (reference "#FLG02") (unit 1)))))
(global_label "COMPUTE_5V" (shape bidirectional) (at 114.30000000000001 243.84 0))
(text "J2 -> Adafruit5206 named pads; VIN=3V3. J5 -> Pololu named pads. J7 -> charger ISET/GND/THERM.\nU1 BAT pads are absent. Remove U1 from sockets before connecting its USB port.\nR4 requires charger factory 1A jumper OPEN. Thermistor requires factory THERM bypass OPEN.\nPower flags declare off-board source/return through J1, J5 and D1; they are not hardware.\nCharge-temperature qualification remains OPEN: native BQ thermistor limits do not prove selected-pack 0..45C compliance." (at 20 270 0))
(sheet_instances (path (page "1")))
)
